(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Handheld Game Console")
    (date "2022-04-15")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../../Downloads/Game Console Manufacturing/")
    )
  )
  (net 0 "")
  (net 1 "+BATT")
  (net 2 "GND")
  (net 3 "+3V3")
  (net 4 "Net-(C4-Pad2)")
  (net 5 "Net-(C5-Pad2)")
  (net 6 "/A")
  (net 7 "/B")
  (net 8 "/X")
  (net 9 "/Y")
  (net 10 "/Up")
  (net 11 "/Down")
  (net 12 "/Left")
  (net 13 "/Right")
  (net 14 "+5V")
  (net 15 "Net-(D2-Pad1)")
  (net 16 "/CS")
  (net 17 "/Clock")
  (net 18 "/Data")
  (net 19 "/LS{slash}DC")
  (net 20 "/RST")
  (net 21 "Net-(D3-Pad3)")
  (net 22 "Net-(J1-PadA5)")
  (net 23 "Net-(J1-PadB5)")
  (net 24 "Net-(Q2-Pad1)")
  (net 25 "Net-(Q2-Pad2)")
  (net 26 "Net-(R1-Pad1)")
  (net 27 "Net-(R3-Pad2)")
  (net 28 "/LEDK")
  (net 29 "unconnected-(U2-Pad4)")
  (net 30 "/D+")
  (net 31 "/D-")
  (net 32 "unconnected-(U3-Pad11)")
  (net 33 "unconnected-(U3-Pad10)")
  (net 34 "unconnected-(U3-Pad8)")
  (net 35 "unconnected-(U3-Pad16)")
  (net 36 "unconnected-(U3-Pad22)")
  (net 37 "unconnected-(U3-Pad23)")
  (net 38 "unconnected-(U3-Pad24)")
  (net 39 "unconnected-(U3-Pad35)")
  (net 40 "unconnected-(U3-Pad36)")
  (net 41 "unconnected-(U3-Pad25)")
  (net 42 "unconnected-(U3-Pad26)")
  (net 43 "unconnected-(J1-PadB8)")
  (net 44 "unconnected-(J1-PadA8)")
  (net 45 "unconnected-(J4-Pad2)")
  (net 46 "unconnected-(J4-Pad6)")
  (net 47 "Net-(D4-Pad1)")
  (net 48 "Net-(D5-Pad1)")
  (net 49 "Net-(D6-Pad1)")
  (net 50 "Net-(D6-Pad2)")
  (net 51 "Net-(D7-Pad1)")
  (net 52 "unconnected-(U3-Pad28)")
  (net 53 "unconnected-(U3-Pad34)")
  (net 54 "unconnected-(U3-Pad33)")
  (net 55 "unconnected-(U3-Pad32)")
  (net 56 "unconnected-(U3-Pad31)")
  (net 57 "unconnected-(U3-Pad30)")
  (net 58 "unconnected-(U3-Pad29)")
  (net 59 "Net-(C2-Pad1)")
  (net 60 "Net-(R4-Pad2)")
  (net 61 "Net-(U2-Pad3)")
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 114.03 89.154)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0.254 1.778) (layer "F.SilkS"))
    (fp_text value "5.1k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 23 "Net-(J1-PadB5)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 124.7355 90.496)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "10 uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 120.142 61.468)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 3.048 0.0296) (layer "F.SilkS"))
    (fp_text value "10 uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 112.776 63.754 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 1.778) (layer "F.SilkS"))
    (fp_text value "10 uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 59 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 160.984 126.202 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW4" (at 3.4544 6.35) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "/A") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "/A") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.462 71.446)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at -0.104 1.706) (layer "F.SilkS"))
    (fp_text value "22R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 25 "Net-(Q2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 21 "Net-(D3-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123F" (layer "F.Cu")
    (tedit 587F7769)
    (at 112.268 67.818 -90)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at -0.254 -2.032 90) (layer "F.SilkS"))
    (fp_text value "D_Schottky" (at 0 2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.127 -1.905 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.4 0 270) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(C2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.4 0 270) (size 1.1 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 125.4545 131.318)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 0 1.778) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 12 "/Left") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 62514183)
    (at 104.14 53.34)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0.762 4.064) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.599999 5.599999) (drill 3.200001) (layers *.Cu *.Mask)
      (net 2 "GND"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.22 63.754 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 2.81 0) (layer "F.SilkS"))
    (fp_text value "60.4R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "Net-(D5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.458 66.294 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.524) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 59 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 60 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 158.7195 117.13)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 6 "/A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "450404015514:450404015514" (layer "F.Cu")
    (tedit 625A2816)
    (at 102.362 67.564 90)
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 0.254 -2.286 90) (layer "F.SilkS"))
    (fp_text value "SW_SPDT" (at 4.92 3.665 90) (layer "F.Fab"))
    (fp_text user "1" (at 3 2.5 90) (layer "F.Fab"))
    (fp_text user "3" (at -3.25 2.5 90) (layer "F.Fab"))
    (fp_text user "2" (at 0.05 2.5 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -1.5 0 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 1.5 0 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "1" smd rect locked (at 2.25 2.05 180) (size 1.1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(R4-Pad2)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect locked (at -0.75 2.05 180) (size 1.1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(U2-Pad3)") (pinfunction "B") (pintype "passive"))
    (pad "3" smd rect locked (at -2.25 2.05 180) (size 1.1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "C") (pintype "passive"))
    (pad "Z1" smd rect locked (at -3.75 -1.15 90) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "Z2" smd rect locked (at 3.75 -1.15 90) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "Z3" smd rect locked (at 3.75 1.15 90) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "Z4" smd rect locked (at -3.75 1.15 90) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "Espressif:ESP32-S2-SOLO" (layer "F.Cu")
    (tedit 60FECD9E)
    (at 147.32 90.794 180)
    (descr "ESP32-S2-SOLO https://www.espressif.com/sites/default/files/documentation/esp32-s2-solo_esp32-s2-solo-u_datasheet_en.pdf")
    (tags "esp32-s2 module")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 8.128 -16.974) (layer "F.SilkS"))
    (fp_text value "ESP32-S2-SOLO" (at 0 12) (layer "F.Fab"))
    (fp_text user "Antenna Area" (at 0 -12.75) (layer "F.SilkS"))
    (fp_text user "Antenna Area" (at 0 -12.75) (layer "Eco2.User"))
    (fp_text user "REF**" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -8.75 -8.26 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect locked (at -8.75 -6.99 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "3V3") (pintype "power_in"))
    (pad "3" smd rect locked (at -8.75 -5.72 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C4-Pad2)") (pinfunction "EN") (pintype "bidirectional"))
    (pad "4" smd rect locked (at -8.75 -4.45 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/Y") (pinfunction "GPIO4/TOUCH4/ADC1_CH3") (pintype "bidirectional"))
    (pad "5" smd rect locked (at -8.75 -3.18 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/Up") (pinfunction "GPIO5/TOUCH5/ADC1_CH4") (pintype "bidirectional"))
    (pad "6" smd rect locked (at -8.75 -1.91 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/Down") (pinfunction "GPIO6/TOUCH6/ADC1_CH5") (pintype "bidirectional"))
    (pad "7" smd rect locked (at -8.75 -0.64 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/Left") (pinfunction "GPIO7/TOUCH7/ADC1_CH6") (pintype "bidirectional"))
    (pad "8" smd rect locked (at -8.75 0.63 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "unconnected-(U3-Pad8)") (pinfunction "GPIO15/U0RTS/ADC2_CH4/XTAL_32K_P") (pintype "bidirectional+no_connect"))
    (pad "9" smd rect locked (at -8.75 1.9 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(D6-Pad2)") (pinfunction "GPIO16/U0CTS/ADC2_CH5/XTAL_32K_N") (pintype "bidirectional"))
    (pad "10" smd rect locked (at -8.75 3.17 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "unconnected-(U3-Pad10)") (pinfunction "GPIO17/U1TXD/ADC2_CH6/DAC_1") (pintype "bidirectional+no_connect"))
    (pad "11" smd rect locked (at -8.75 4.44 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "unconnected-(U3-Pad11)") (pinfunction "GPIO18/U1RXD/ADC2_CH7/DAC_2/CLK_OUT3") (pintype "bidirectional+no_connect"))
    (pad "12" smd rect locked (at -8.75 5.71 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/Right") (pinfunction "GPIO8/TOUCH8/ADC1_CH7") (pintype "bidirectional"))
    (pad "13" smd rect locked (at -8.75 6.98 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/D-") (pinfunction "GPIO19/U1RTS/ADC2_CH8/CLK_OUT2/USB_D-") (pintype "bidirectional"))
    (pad "14" smd rect locked (at -8.75 8.25 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/D+") (pinfunction "GPIO20/U1CTS/ADC2_CH9/CLK_OUT1/USB_D+") (pintype "bidirectional"))
    (pad "15" smd rect locked (at -6.985 9.5 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/X") (pinfunction "GPIO3/TOUCH3/ADC1_CH2") (pintype "bidirectional"))
    (pad "16" smd rect locked (at -5.715 9.5 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "unconnected-(U3-Pad16)") (pinfunction "GPIO46") (pintype "input+no_connect"))
    (pad "17" smd rect locked (at -4.445 9.5 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/CS") (pinfunction "GPIO9/TOUCH9/ADC1_CH8/FSPIHD") (pintype "bidirectional"))
    (pad "18" smd rect locked (at -3.175 9.5 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/Data") (pinfunction "GPIO10/TOUCH10/ADC1_CH9/FSPICS0/FSPIIO4") (pintype "bidirectional"))
    (pad "19" smd rect locked (at -1.905 9.5 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/LS{slash}DC") (pinfunction "GPIO11/TOUCH11/ADC2_CH0/FSPID/FSPIIO5") (pintype "bidirectional"))
    (pad "20" smd rect locked (at -0.635 9.5 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/RST") (pinfunction "GPIO12/TOUCH12/ADC2_CH1/FSPICLK/FSPIIO6") (pintype "bidirectional"))
    (pad "21" smd rect locked (at 0.635 9.5 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/LEDK") (pinfunction "GPIO13/TOUCH13/ADC2_CH2/FSPIQ/FSPIIO7") (pintype "bidirectional"))
    (pad "22" smd rect locked (at 1.905 9.5 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "unconnected-(U3-Pad22)") (pinfunction "GPIO14/TOUCH14/ADC2_CH3/FSPIWP/FSPIDQS") (pintype "bidirectional+no_connect"))
    (pad "23" smd rect locked (at 3.175 9.5 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "unconnected-(U3-Pad23)") (pinfunction "GPIO21") (pintype "bidirectional+no_connect"))
    (pad "24" smd rect locked (at 4.445 9.5 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "unconnected-(U3-Pad24)") (pinfunction "SPIIO4/GPIO33/FSPIHD") (pintype "bidirectional+no_connect"))
    (pad "25" smd rect locked (at 5.715 9.5 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "unconnected-(U3-Pad25)") (pinfunction "SPIIO5/GPIO34/FSPICS0") (pintype "bidirectional+no_connect"))
    (pad "26" smd rect locked (at 6.985 9.5 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "unconnected-(U3-Pad26)") (pinfunction "GPIO45") (pintype "bidirectional+no_connect"))
    (pad "27" smd rect locked (at 8.75 8.25) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(C5-Pad2)") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "28" smd rect locked (at 8.75 6.98) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "unconnected-(U3-Pad28)") (pinfunction "SPIIO6/GPIO35/FSPID") (pintype "bidirectional+no_connect"))
    (pad "29" smd rect locked (at 8.75 5.71) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "unconnected-(U3-Pad29)") (pinfunction "SPIIO7/GPIO36/FSPICLK") (pintype "bidirectional+no_connect"))
    (pad "30" smd rect locked (at 8.75 4.44) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "unconnected-(U3-Pad30)") (pinfunction "SPIDQS/GPIO37/FSPIQ") (pintype "bidirectional+no_connect"))
    (pad "31" smd rect locked (at 8.75 3.17) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "unconnected-(U3-Pad31)") (pinfunction "GPIO38/FSPIWP") (pintype "bidirectional+no_connect"))
    (pad "32" smd rect locked (at 8.75 1.9) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "unconnected-(U3-Pad32)") (pinfunction "MTCK/GPIO39/CLK_OUT3") (pintype "bidirectional+no_connect"))
    (pad "33" smd rect locked (at 8.75 0.63) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "unconnected-(U3-Pad33)") (pinfunction "MTDO/GPIO40/CLK_OUT2") (pintype "bidirectional+no_connect"))
    (pad "34" smd rect locked (at 8.75 -0.64) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "unconnected-(U3-Pad34)") (pinfunction "MTDI/GPIO41/CLK_OUT1") (pintype "bidirectional+no_connect"))
    (pad "35" smd rect locked (at 8.75 -1.91) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "unconnected-(U3-Pad35)") (pinfunction "MTMS/GPIO42") (pintype "bidirectional+no_connect"))
    (pad "36" smd rect locked (at 8.75 -3.18) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "unconnected-(U3-Pad36)") (pinfunction "U0RXD/GPIO44/CLK_OUT2") (pintype "bidirectional+no_connect"))
    (pad "37" smd rect locked (at 8.75 -4.45) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/Clock") (pinfunction "U0TXD/GPIO43/CLK_OUT1") (pintype "bidirectional"))
    (pad "38" smd rect locked (at 8.75 -5.72) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/B") (pinfunction "GPIO2/TOUCH2/ADC1_CH1") (pintype "bidirectional"))
    (pad "39" smd rect locked (at 8.75 -6.99) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/A") (pinfunction "GPIO1/TOUCH1/ADC1_CH0") (pintype "bidirectional"))
    (pad "40" smd rect locked (at 8.75 -8.26) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "41" smd rect locked (at -2.9 -0.54) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "41" smd rect locked (at -1.5 -1.94) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "41" smd rect locked (at -2.9 -1.94) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "41" smd rect locked (at -1.5 0.86) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "41" smd rect locked (at -2.9 0.86) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "41" smd rect locked (at -1.5 -0.54) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "41" smd rect locked (at -0.1 -0.54) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "41" smd rect locked (at -0.1 0.86) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "41" smd rect locked (at -0.1 -1.94) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 108.712 79.502)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at -2.032 -0.508) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 14 "+5V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 102.87 77.47)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 3.556 0) (layer "F.SilkS"))
    (fp_text value "140R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 51 "Net-(D7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 117.094 70.866)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 2.286 0) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 1 "+BATT") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 106.68 117.856)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 13 "/Right") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 135.18 121.702)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW6" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "/X") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "/X") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 144.78 130.846)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW7" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "/Y") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 "/Y") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.714 92.782 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 3.048 -0.436) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 15 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 27 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 118.82 117.566 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW9" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "/Down") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "/Down") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 118.82 134.838 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW10" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "/Left") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "/Left") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.032 85.924 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 26 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 108.22 61.214)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at -3.048 0) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 48 "Net-(D5-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 3 "+3V3") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.745 80.01 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "82R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 47 "Net-(D4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 124.968 85.924)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.4) (layer "F.SilkS"))
    (fp_text value "MCP73831-2-OT" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(R3-Pad2)") (pinfunction "STAT") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pinfunction "VBAT") (pintype "power_out"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(R1-Pad1)") (pinfunction "PROG") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 124.46 116.332)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 10 "/Up") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 144.78 112.558)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW5" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "/B") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "/B") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 115.01 103.196 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(C4-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 138.632 130.8245 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 8 "/X") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 161.29 91.44)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 1.524) (layer "F.SilkS"))
    (fp_text value "60.4R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 49 "Net-(D6-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 118.745 76.835 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0 -1.778 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 47 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "+BATT") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 6251411F)
    (at 160.02 139.7)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.8) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3_DIN965_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.599999 5.599999) (drill 3.200001) (layers *.Cu *.Mask)
      (net 2 "GND"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 125.222 107.514)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 1.706 180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 5 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.506 76.272)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0.658 1.96) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 14 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 625243C1)
    (at 157.48 52.07)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.54 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x10" (at 0 25.19) (layer "F.Fab"))
    (fp_text user "LITE" (at 3.048 0 unlocked) (layer "F.SilkS"))
    (fp_text user "SCK" (at 3.302 5.08 unlocked) (layer "F.SilkS"))
    (fp_text user "TFT_CS" (at 4.318 10.16 unlocked) (layer "F.SilkS"))
    (fp_text user "CARD" (at 4.064 12.7 unlocked) (layer "F.SilkS"))
    (fp_text user "RESET" (at 4.318 17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "VCC" (at 3.556 20.32 unlocked) (layer "F.SilkS"))
    (fp_text user "MOSI" (at 3.556 7.62 unlocked) (layer "F.SilkS"))
    (fp_text user "MISO" (at 3.556 2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "GND" (at 3.81 22.86 unlocked) (layer "F.SilkS"))
    (fp_text user "D/C" (at 3.556 15.24 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 11.43 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/LEDK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "unconnected-(J4-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/Clock") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/Data") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/CS") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "unconnected-(J4-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/LS{slash}DC") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/RST") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+3V3") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 111.506 72.39 180)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at -3.81 -1.27 180) (layer "F.SilkS"))
    (fp_text value "SSM3J331R,LF" (at 0 2.5 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "+5V") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(C2-Pad1)") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect (at 1.5 0 180) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+BATT") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 138.378 115.352)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 7 "/B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "USB4500-03-0-A_REVA:GCT_USB4500-03-0-A_REVA" (layer "F.Cu")
    (tedit 6250DEAA)
    (at 100.832 86.497 -90)
    (property "MANUFACTURER" "GCT")
    (property "MAXIMUM_PACKAGE_HEIGHT" "2.46mm")
    (property "PARTREV" "A")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -0.065 -3.1035 90) (layer "F.SilkS"))
    (fp_text value "USB4500-03-0-A_REVA" (at 9.155 -7.385 90) (layer "F.Fab"))
    (fp_text user "PCB-Edge" (at 9.769 1.3185 -90) (layer "F.Fab"))
    (pad "A1_B12" smd rect (at -3.2 -5.15 270) (size 0.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_A") (pintype "power_in"))
    (pad "A4_B9" smd rect (at -2.4 -5.15 270) (size 0.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "+5V") (pinfunction "VBUS_A") (pintype "power_in"))
    (pad "A5" smd rect (at -1.25 -5.15 270) (size 0.3 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(J1-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.25 -5.15 270) (size 0.3 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/D+") (pinfunction "DP1") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.25 -5.15 270) (size 0.3 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/D-") (pinfunction "DN1") (pintype "bidirectional"))
    (pad "A8" smd rect (at 1.25 -5.15 270) (size 0.3 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "unconnected-(J1-PadA8)") (pinfunction "SBU1") (pintype "bidirectional+no_connect"))
    (pad "B1_A12" smd rect (at 3.2 -5.15 270) (size 0.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND_B") (pintype "power_in"))
    (pad "B4_A9" smd rect (at 2.4 -5.15 270) (size 0.6 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "+5V") (pinfunction "VBUS_B") (pintype "power_in"))
    (pad "B5" smd rect (at 1.75 -5.15 270) (size 0.3 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(J1-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect (at 0.75 -5.15 270) (size 0.3 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/D+") (pinfunction "DP2") (pintype "bidirectional"))
    (pad "B7" smd rect (at -0.75 -5.15 270) (size 0.3 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/D-") (pinfunction "DN2") (pintype "bidirectional"))
    (pad "B8" smd rect (at -1.75 -5.15 270) (size 0.3 1.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "unconnected-(J1-PadB8)") (pinfunction "SBU2") (pintype "bidirectional+no_connect"))
    (pad "S1" thru_hole oval (at -5.62 0 270) (size 0.95 1.9) (drill oval 0.6 1.8) (layers *.Cu)
      (net 2 "GND") (pinfunction "SHELL_GND") (pintype "power_in"))
    (pad "S2" thru_hole oval (at 5.62 -4 270) (size 0.8 1.6) (drill oval 0.6 1.4) (layers *.Cu)
      (net 2 "GND") (pinfunction "SHELL_GND") (pintype "power_in"))
    (pad "S3" thru_hole oval (at -5.62 -4 270) (size 0.8 1.6) (drill oval 0.6 1.4) (layers *.Cu)
      (net 2 "GND") (pinfunction "SHELL_GND") (pintype "power_in"))
    (pad "S4" thru_hole oval (at 5.62 0 270) (size 0.95 1.9) (drill oval 0.6 1.8) (layers *.Cu)
      (net 2 "GND") (pinfunction "SHELL_GND") (pintype "power_in"))
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 121.972 98.914)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW3" (at -2.084 2.178) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 129.54 91.512 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 15 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 14 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 127.456 126.202 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW8" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "/Up") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "/Up") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H5mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 110.184 126.202 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW11" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "/Right") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "/Right") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-523" (layer "F.Cu")
    (tedit 5E27725A)
    (at 137.414 69.16 90)
    (descr "SOT523, https://www.diodes.com/assets/Package-Files/SOT523.pdf")
    (tags "SOT-523")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q2" (at 2.612 0.15 180) (layer "F.SilkS"))
    (fp_text value "MMBT2222AT-7-F" (at 0 1.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.645 -0.5 270) (size 0.51 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(Q2-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd rect (at -0.645 0.5 270) (size 0.51 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(Q2-Pad2)") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 0.645 0 270) (size 0.51 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-523.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "XC6210B332MR-G:IC_XC8107AC20MR-G" (layer "F.Cu")
    (tedit 6259E960)
    (at 117.475 64.77)
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at -0.635 -2.54) (layer "F.SilkS"))
    (fp_text value "XC6210B332MR" (at 8.205 2.525) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.2 -0.95) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(C2-Pad1)") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd rect locked (at -1.2 0) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect locked (at -1.2 0.95) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(U2-Pad3)") (pinfunction "CE") (pintype "input"))
    (pad "4" smd rect locked (at 1.2 0.95) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "unconnected-(U2-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect locked (at 1.2 -0.95) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "VOUT") (pintype "power_out"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad" (layer "F.Cu")
    (tedit 62513E41)
    (at 104.14 139.7)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.85) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3_ISO7380_Pad" (at 0 3.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 "GND"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 136.144 73.224 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 28 "/LEDK") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 24 "Net-(Q2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 157.428 130.592)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 9 "/Y") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 161.29 88.9 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at 0 1.778) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 49 "Net-(D6-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 50 "Net-(D6-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 102.87 74.93)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D7" (at -0.254 -1.778) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 51 "Net-(D7-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 14 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.522 84.328)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at -0.227064 -1.524) (layer "F.SilkS"))
    (fp_text value "5.1k" (at 0 1.65) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 22 "Net-(J1-PadA5)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 121.92 63.754)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 3.5345 0) (layer "F.SilkS"))
    (fp_text value "1 uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 115.824 109.982)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at -3.556 0) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 11 "/Down") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "JD-T1800:JD-T1800" (layer "F.Cu")
    (tedit 62593F91)
    (at 137.16 65.858009 90)
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at 4.898 10.922) (layer "F.SilkS"))
    (fp_text value "JD-T1800" (at 0 10.16 90) (layer "F.Fab"))
    (fp_text user "1" (at 6.604 12.954 unlocked) (layer "F.SilkS"))
    (fp_text user "14" (at -6.35 12.954 unlocked) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 7.65 16.9 90) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -12.8 16.9 90) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" smd rect (at 5.2 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at 4.4 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at 3.6 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(D3-Pad3)") (pinfunction "LEDK") (pintype "input"))
    (pad "4" smd rect (at 2.8 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "LEDA") (pintype "input"))
    (pad "5" smd rect (at 2 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND1") (pintype "power_in"))
    (pad "6" smd rect (at 1.2 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/RST") (pinfunction "RESET") (pintype "input"))
    (pad "7" smd rect (at 0.4 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/LS{slash}DC") (pinfunction "RS/DC") (pintype "input"))
    (pad "8" smd rect (at -0.4 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/Data") (pinfunction "DATA") (pintype "input"))
    (pad "9" smd rect (at -1.2 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/Clock") (pinfunction "CLOCK") (pintype "input"))
    (pad "10" smd rect (at -2 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "11" smd rect (at -2.8 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+3V3") (pinfunction "VCC2") (pintype "power_in"))
    (pad "12" smd rect (at -3.6 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/CS") (pinfunction "CS") (pintype "input"))
    (pad "13" smd rect (at -4.4 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND2") (pintype "power_in"))
    (pad "14" smd rect (at -5.2 13.1 180) (size 2 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 111.506 58.166)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 3 "+3V3") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 112.268 94.814)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal" (layer "B.Cu")
    (tedit 5B78AD87)
    (at 121.92 55.88 -90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at -5.588 0.58) (layer "B.SilkS"))
    (fp_text value "Conn_01x02" (at 0 -5.8 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5 -270) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 2.85 270) (size 1 3.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+BATT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 2.85 270) (size 1 3.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "MP" smd roundrect (at -3.35 -2.9 270) (size 1.5 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1666673333))
    (pad "MP" smd roundrect (at 3.35 -2.9 270) (size 1.5 3.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1666673333))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 148.082 95.758)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 1.778) (layer "B.SilkS"))
    (fp_text value "10k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2083333333)
      (net 4 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 152.64325 98.806 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 3.302 0.254 90) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 150.114 98.806 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Game Console.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 3.4305 -0.182 90) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 3 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 165.1 53.34) (end 165.1 139.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 104.14 48.26) (end 160.02 48.26) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 160.02 48.26) (mid 163.612102 49.747898) (end 165.1 53.34) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 104.14 144.78) (mid 100.547898 143.292102) (end 99.06 139.7) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 165.1 139.7) (mid 163.612102 143.292102) (end 160.02 144.78) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 160.02 144.78) (end 104.14 144.78) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 99.06 53.34) (mid 100.547898 49.747898) (end 104.14 48.26) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.06 139.7) (end 99.06 53.34) (layer "Edge.Cuts") (width 0.1))
  (gr_text "HOPE 2022" (at 112.014 50.038) (layer "F.SilkS"))
  (gr_text "+3.3V\n" (at 107.95 58.674) (layer "F.SilkS"))
  (gr_text "Test\n" (at 161.29 85.852) (layer "F.SilkS"))
  (gr_text "PCB-Boy 1.0" (at 113.538 142.748) (layer "F.SilkS"))
  (gr_text "GPIO0" (at 124.968 105.664) (layer "F.SilkS"))
  (gr_text "EN\n" (at 111.76 106.68) (layer "F.SilkS"))
  (gr_text "Batt. Charge\n" (at 131.064 91.694 90) (layer "F.SilkS"))
  (gr_text "+VBatt\n" (at 118.872 75.184) (layer "F.SilkS"))
  (gr_text "+5V\n" (at 100.33 75.184 90) (layer "F.SilkS"))
  (gr_text "Kevin He, Kesava Viswanadha, Ryan Ma" (at 141.986 142.748) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.3048) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 147.32)
        (xy 96.52 147.32)
        (xy 96.52 45.72)
        (xy 167.64 45.72)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.3048) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 147.32)
        (xy 96.52 147.32)
        (xy 96.52 45.72)
        (xy 167.64 45.72)
      )
    )
  )
)
