(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plots/")
    )
  )
  (net 0 "")
  (net 1 "+15V")
  (net 2 "GND")
  (net 3 "+5V")
  (net 4 "Net-(U1-VD)")
  (net 5 "Net-(U1-BST)")
  (net 6 "+3V3")
  (net 7 "/MOTOR_PS1")
  (net 8 "/MOTOR_PS2")
  (net 9 "Net-(U1-ON{slash}~{OFF})")
  (net 10 "unconnected-(U2-NC-Pad4)")
  (net 11 "Net-(D1-C)")
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 158.75 74.87 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "1M" (at 11.366 25.58425 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 1 "+15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 9 "Net-(U1-ON{slash}~{OFF})") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PDB_Diode:DIOM5226X230N" (layer "F.Cu")
    (at 148.104 75.3375 90)
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Schottky diode")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D1" (at -0.635 -3.175 90) (layer "F.SilkS") hide)
    (fp_text value "D_Schottky" (at 4.445 3.175 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -2.135 0 90) (size 2.33 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D1-C)") (pinfunction "C") (pintype "passive"))
    (pad "2" smd rect (at 2.135 0 90) (size 2.33 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KIPRJMOD}/parts/SMA_DIO.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 158.75 79.105 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "130k" (at 11.366 25.58425 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 9 "Net-(U1-ON{slash}~{OFF})") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (layer "F.Cu")
    (at 123.7996 87.2744)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "B.Cu" "B.Mask"))
  )
  (footprint "Capacitor_SMD:C_01005_0402Metric_Pad0.57x0.30mm_HandSolder" (layer "F.Cu")
    (at 149.606 80.45 90)
    (descr "Capacitor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C_IN2" (at 0 -1 90) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.3625 0 90) (size 0.41 0.27) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.3625 0 90) (size 0.41 0.27) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.3375 0 90) (size 0.575 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(U1-BST)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.3375 0 90) (size 0.575 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D1-C)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "2_Pin:215760-YY02" (layer "F.Cu")
    (at 163.11 65.4 180)
    (descr "215760-YY02")
    (tags "Connector")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MOTOR" (at 2.836 3.8304 90) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at -1.5 4.3 180) (size 3 3) (drill 3) (layers "F&B.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 7 "/MOTOR_PS1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -3 0 180) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/parts/2157601002.stp"
      (offset (xyz -1.5 -4 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_01005_0402Metric_Pad0.57x0.30mm_HandSolder" (layer "F.Cu")
    (at 131.3365 62.992 180)
    (descr "Capacitor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C_IN4" (at 0 -1) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.3625 0 180) (size 0.41 0.27) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.3625 0 180) (size 0.41 0.27) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.3375 0 180) (size 0.575 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.3375 0 180) (size 0.575 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_01005_0402Metric_Pad0.57x0.30mm_HandSolder" (layer "F.Cu")
    (at 133.01 67.564)
    (descr "Capacitor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C_IN3" (at 0 -1) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.3625 0) (size 0.41 0.27) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.3625 0) (size 0.41 0.27) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.3375 0) (size 0.575 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.3375 0) (size 0.575 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "2_Pin:215760-YY02" (layer "F.Cu")
    (at 128.778 80.216 -90)
    (descr "215760-YY02")
    (tags "Connector")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text value "+5V" (at 3.096 2.667) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at -1.5 4.3 270) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -3 0 270) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/parts/2157601002.stp"
      (offset (xyz -1.5 -4 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "2_Pin:215760-YY02" (layer "F.Cu")
    (at 128.778 70.612 -90)
    (descr "215760-YY02")
    (tags "Connector")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at -0.762 -3.302 90) (layer "F.SilkS") hide)
    (fp_text value "+3V3" (at 3.302 3.302) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at -1.5 4.3 270) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 6 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -3 0 270) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/parts/2157601002.stp"
      (offset (xyz -1.5 -4 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (layer "F.Cu")
    (at 171.0944 87.2744)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "B.Cu" "B.Mask"))
  )
  (footprint "LDO_Regulator:SOT95P280X145-5N" (layer "F.Cu")
    (at 134.3 64.245 90)
    (property "MANUFACTURER" "Texas Instruments")
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.45mm")
    (property "PARTREV" "F")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at -0.06 -2.508 90) (layer "F.SilkS") hide)
    (fp_text value "5V TO 3V3 LDO" (at 3.031 0.234 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.255 -0.95 90) (size 1.21 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 3 "+5V") (pinfunction "IN") (pintype "input"))
    (pad "2" smd roundrect (at -1.255 0 90) (size 1.21 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect (at 0 0 90) (size 0.75 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (thermal_bridge_angle 45))
    (pad "3" smd roundrect (at -1.255 0.95 90) (size 1.21 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 3 "+5V") (pinfunction "EN") (pintype "input"))
    (pad "4" smd roundrect (at 1.255 0.95 90) (size 1.21 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 10 "unconnected-(U2-NC-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at 1.255 -0.95 90) (size 1.21 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15)
      (net 6 "+3V3") (pinfunction "OUT") (pintype "output"))
    (model "${KIPRJMOD}/parts/TLV71333PDBVR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "6_Pin:2125280601" (layer "F.Cu")
    (at 166.116 70.866 90)
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -2.995005 2.809999 90) (layer "F.SilkS") hide)
    (fp_text value "POWER SUPPLY" (at -2.995005 -5.08 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0 0 90) (layer "F.SilkS"))
    (fp_text user "*" (at 0 0 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.999999 4.299999 90) (size 3 3) (drill 3) (layers "F&B.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.52 1.52) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at -2.999999 0 90) (size 1.52 1.52) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at -5.999998 0 90) (size 1.52 1.52) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 0 -2.999999 180) (size 1.52 1.52) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 7 "/MOTOR_PS1") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole circle (at -2.999999 -2.999999 90) (size 1.52 1.52) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 1 "+15V") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at -5.999998 -2.999999 90) (size 1.52 1.52) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 8 "/MOTOR_PS2") (pinfunction "6") (pintype "unspecified"))
    (model "${KIPRJMOD}/parts/2125280601.stp"
      (offset (xyz -3 -8.9 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Switching_Regulator:SOIC127P600X175-8N" (layer "F.Cu")
    (at 153.035 80.453 90)
    (property "AVAILABILITY" "Unavailable")
    (property "DESCRIPTION" "Conv DC-DC Single Step Down 7.5V to 76V 8-Pin SOIC N")
    (property "MF" "Maxim Integrated")
    (property "MP" "MAX5033BASA+T")
    (property "PACKAGE" "SOIC-8 Maxim Integrated")
    (property "PRICE" "None")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -0.795 -3.332 90) (layer "F.SilkS") hide)
    (fp_text value "16V TO 5V" (at 0 3.57 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 90) (size 1.97 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 5 "Net-(U1-BST)") (pinfunction "BST") (pintype "passive"))
    (pad "2" smd roundrect (at -2.475 -0.635 90) (size 1.97 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 4 "Net-(U1-VD)") (pinfunction "VD") (pintype "output"))
    (pad "3" smd roundrect (at -2.475 0.635 90) (size 1.97 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 2 "GND") (pinfunction "SGND") (pintype "power_in"))
    (pad "4" smd roundrect (at -2.475 1.905 90) (size 1.97 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 3 "+5V") (pinfunction "FB") (pintype "input"))
    (pad "5" smd roundrect (at 2.475 1.905 90) (size 1.97 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 9 "Net-(U1-ON{slash}~{OFF})") (pinfunction "ON/~{OFF}") (pintype "input"))
    (pad "6" thru_hole circle (at -0.5 -1.5 90) (size 0.6 0.6) (drill 0.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole circle (at -0.5 -0.5 90) (size 0.6 0.6) (drill 0.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole circle (at -0.5 0.5 90) (size 0.6 0.6) (drill 0.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole circle (at -0.5 1.5 90) (size 0.6 0.6) (drill 0.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd rect (at 0 0 90) (size 2 4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (thermal_bridge_angle 45))
    (pad "6" thru_hole circle (at 0.5 -1.5 90) (size 0.6 0.6) (drill 0.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole circle (at 0.5 -0.5 90) (size 0.6 0.6) (drill 0.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole circle (at 0.5 0.5 90) (size 0.6 0.6) (drill 0.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole circle (at 0.5 1.5 90) (size 0.6 0.6) (drill 0.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 0.635 90) (size 1.97 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd roundrect (at 2.475 -0.635 90) (size 1.97 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 1 "+15V") (pinfunction "VIN") (pintype "input"))
    (pad "8" smd roundrect (at 2.475 -1.905 90) (size 1.97 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 11 "Net-(D1-C)") (pinfunction "LX") (pintype "passive"))
    (model "${KIPRJMOD}/parts/21-0041B_8_MXM.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Bourns_SRR1260" (layer "F.Cu")
    (at 139.446 82.32 -90)
    (descr "Bourns SRR1260 series SMD inductor http://www.bourns.com/docs/Product-Datasheets/SRR1260.pdf")
    (tags "Bourns SRR1260 SMD inductor")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr smd)
    (fp_text reference "L1" (at 0 -7.25 90) (layer "F.SilkS") hide)
    (fp_text value "220uH" (at 0 7.4 90) (layer "F.Fab") hide)
    (pad "1" smd rect (at -4.85 0 270) (size 2.9 5.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D1-C)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 4.85 0 270) (size 2.9 5.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRR1260.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_01005_0402Metric_Pad0.57x0.30mm_HandSolder" (layer "F.Cu")
    (at 152.4 85.4525 -90)
    (descr "Capacitor SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C_IN1" (at 0 -1 90) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1 90) (layer "F.Fab") hide)
    (pad "" smd roundrect (at -0.3625 0 270) (size 0.41 0.27) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.3625 0 270) (size 0.41 0.27) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -0.3375 0 270) (size 0.575 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(U1-VD)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.3375 0 270) (size 0.575 0.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_01005_0402Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D_Pad2.25x2.55mm_HandSolder" (layer "F.Cu")
    (at 137.541 71.374)
    (descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor, small symbol")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 -3.1) (layer "F.SilkS") hide)
    (fp_text value "33uF" (at 0 3.1) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -3.2 0) (size 2.25 2.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 3.2 0) (size 2.25 2.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (layer "F.Cu")
    (at 123.8504 60.452)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "B.Cu" "B.Mask"))
  )
  (footprint "2_Pin:215760-YY02" (layer "F.Cu")
    (at 166.12 82.34)
    (descr "215760-YY02")
    (tags "Connector")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MOTOR" (at -5.8968 3.9692 90) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at -1.5 4.3) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 8 "/MOTOR_PS2") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -3 0) (size 1.52 1.52) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/parts/2157601002.stp"
      (offset (xyz -1.5 -4 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (layer "F.Cu")
    (at 171.0944 60.452)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "B.Cu" "B.Mask"))
  )
  (footprint "Capacitor_SMD:C_Elec_8x10.2" (layer "F.Cu")
    (at 155.09 68.6 90)
    (descr "SMD capacitor, aluminum electrolytic nonpolar, 8.0x10.2mm")
    (tags "capacitor electrolyic nonpolar")
    (property "Sheetfile" "Power Distribution Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor, small symbol")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 -5.2 90) (layer "F.SilkS") hide)
    (fp_text value "100uF" (at 0 5.2 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -3.6 0 90) (size 4.5 2.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1190480952)
      (net 1 "+15V") (pintype "passive"))
    (pad "2" smd roundrect (at 3.6 0 90) (size 4.5 2.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1190480952)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_8x10.2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Elevate_Logo:ElevateLogo" (layer "B.Cu")
    (at 147.447 63.373 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "Elevate_Logo:ElevateLogo" (layer "B.Cu")
    (at 147.447 73.787 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "Elevate_Logo:ElevateLogo" (layer "B.Cu")
    (at 147.447 84.328 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (gr_line (start 171.0944 89.6112) (end 123.7996 89.6112)
    (layer "Edge.Cuts"))
  (gr_line (start 121.4628 87.2744) (end 121.4628 60.452)
    (layer "Edge.Cuts"))
  (gr_arc (start 121.4628 60.452) (mid 122.147233 58.799633) (end 123.7996 58.1152)
    (layer "Edge.Cuts"))
  (gr_arc (start 123.7996 89.6112) (mid 122.147233 88.926767) (end 121.4628 87.2744)
    (layer "Edge.Cuts"))
  (gr_arc (start 173.4312 87.2744) (mid 172.746767 88.926767) (end 171.0944 89.6112)
    (layer "Edge.Cuts"))
  (gr_arc (start 171.0944 58.1152) (mid 172.746767 58.799633) (end 173.4312 60.452)
    (layer "Edge.Cuts"))
  (gr_line (start 173.4312 60.452) (end 173.4312 87.2744)
    (layer "Edge.Cuts"))
  (gr_line (start 123.7996 58.1152) (end 171.0944 58.1152)
    (layer "Edge.Cuts"))
  (zone (net 11) (net_name "Net-(D1-C)") (layer "F.Cu") (name "1") (hatch none 0.5)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 1) (smoothing fillet) (radius 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 151.638 79.121)
        (xy 136.398 79.121)
        (xy 136.398 75.819)
        (xy 151.638 75.819)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (name "GND") (hatch none 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 1) (smoothing fillet) (radius 3) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 127.254 60.452)
        (xy 127.254 87.376)
        (xy 167.64 87.376)
        (xy 167.64 60.452)
      )
    )
  )
)
