(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "74AHC04_1" (in_bom yes) (on_board yes)
      (property "Reference" "U1" (at -7.62 0 0))
      (property "Value" "74AHC04" (at -5.08 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT04.pdf" (at -8.89 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "AHCMOS not inv" (at 0 0 0))
      (property "ki_description" "Hex Inverter" (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm* SSOP?14* TSSOP?14*" (at 0 0 0))
      (symbol "74AHC04_1_1_0"
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy 2.54 0)
            (xy 0 1.27)
          )
          (fill (type background))
        )
        (pin input line (at -3.81 0 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin output inverted (at 6.35 0 180) (length 3.81)
          (name "~")
          (number "2")
        )
      )
      (symbol "74AHC04_1_2_0"
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy 2.54 0)
            (xy 0 1.27)
          )
          (fill (type background))
        )
        (pin input line (at -3.81 0 0) (length 3.81)
          (name "~")
          (number "3")
        )
        (pin output inverted (at 6.35 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
      )
      (symbol "74AHC04_1_3_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74AHC04_1_4_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74AHC04_1_5_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "11")
        )
      )
      (symbol "74AHC04_1_6_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74AHC04_1_7_0"
        (pin power_in line (at -1.27 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at -1.27 -7.62 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74AHC04_1_7_1"
        (rectangle (start -5.08 7.62) (end 2.54 -2.54)
          (fill (type background))
        )
      )
    )
    (symbol "74AHC04_2" (in_bom yes) (on_board yes)
      (property "Reference" "U1C" (at 0 5.08 0))
      (property "Value" "74AHC04" (at 0 2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT04.pdf" (at 0 -8.89 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "AHCMOS not inv" (at 0 0 0))
      (property "ki_description" "Hex Inverter" (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm* SSOP?14* TSSOP?14*" (at 0 0 0))
      (symbol "74AHC04_2_1_0"
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy 2.54 0)
            (xy 0 1.27)
          )
          (fill (type background))
        )
        (pin input line (at -3.81 0 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin output inverted (at 6.35 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74AHC04_2_2_0"
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy 2.54 0)
            (xy 0 1.27)
          )
          (fill (type background))
        )
        (pin input line (at -3.81 0 0) (length 3.81)
          (name "~")
          (number "3")
        )
        (pin output inverted (at 6.35 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
      )
      (symbol "74AHC04_2_3_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74AHC04_2_4_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74AHC04_2_5_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "11")
        )
      )
      (symbol "74AHC04_2_6_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74AHC04_2_7_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74AHC04_2_7_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "74AHC04_3" (in_bom yes) (on_board yes)
      (property "Reference" "U3" (at 0 -5.08 0))
      (property "Value" "74AHC04" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT04.pdf" (at 0 -8.89 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "AHCMOS not inv" (at 0 0 0))
      (property "ki_description" "Hex Inverter" (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm* SSOP?14* TSSOP?14*" (at 0 0 0))
      (symbol "74AHC04_3_1_0"
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy 2.54 0)
            (xy 0 1.27)
          )
          (fill (type background))
        )
        (pin input line (at -3.81 0 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin output inverted (at 6.35 0 180) (length 3.81)
          (name "~")
          (number "2")
        )
      )
      (symbol "74AHC04_3_2_0"
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy 2.54 0)
            (xy 0 1.27)
          )
          (fill (type background))
        )
        (pin input line (at -3.81 0 0) (length 3.81)
          (name "~")
          (number "7")
        )
        (pin output inverted (at 6.35 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
      )
      (symbol "74AHC04_3_3_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74AHC04_3_4_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74AHC04_3_5_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "11")
        )
      )
      (symbol "74AHC04_3_6_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74AHC04_3_7_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74AHC04_3_7_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "74AHC04_4" (in_bom yes) (on_board yes)
      (property "Reference" "U1" (at -7.62 0 0))
      (property "Value" "74AHC04" (at -5.08 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT04.pdf" (at -8.89 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "AHCMOS not inv" (at 0 0 0))
      (property "ki_description" "Hex Inverter" (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm* SSOP?14* TSSOP?14*" (at 0 0 0))
      (symbol "74AHC04_4_1_0"
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy 2.54 0)
            (xy 0 1.27)
          )
          (fill (type background))
        )
        (pin input line (at -3.81 0 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin output inverted (at 6.35 0 180) (length 3.81)
          (name "~")
          (number "2")
        )
      )
      (symbol "74AHC04_4_2_0"
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy 2.54 0)
            (xy 0 1.27)
          )
          (fill (type background))
        )
        (pin input line (at -3.81 0 0) (length 3.81)
          (name "~")
          (number "3")
        )
        (pin output inverted (at 6.35 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
      )
      (symbol "74AHC04_4_3_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74AHC04_4_4_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74AHC04_4_5_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "11")
        )
      )
      (symbol "74AHC04_4_6_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74AHC04_4_7_0"
        (pin power_in line (at -1.27 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at -1.27 -7.62 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74AHC04_4_7_1"
        (rectangle (start -5.08 7.62) (end 2.54 -2.54)
          (fill (type background))
        )
      )
    )
    (symbol "74xx:74AHC04" (in_bom yes) (on_board yes)
      (property "Reference" "U1" (at -7.62 0 0))
      (property "Value" "74AHC04" (at -5.08 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT04.pdf" (at -8.89 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "AHCMOS not inv" (at 0 0 0))
      (property "ki_description" "Hex Inverter" (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm* SSOP?14* TSSOP?14*" (at 0 0 0))
      (symbol "74AHC04_1_0"
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy 2.54 0)
            (xy 0 1.27)
          )
          (fill (type background))
        )
        (pin input line (at -3.81 0 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin output inverted (at 6.35 0 180) (length 3.81)
          (name "~")
          (number "2")
        )
      )
      (symbol "74AHC04_2_0"
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy 2.54 0)
            (xy 0 1.27)
          )
          (fill (type background))
        )
        (pin input line (at -3.81 0 0) (length 3.81)
          (name "~")
          (number "3")
        )
        (pin output inverted (at 6.35 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
      )
      (symbol "74AHC04_3_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74AHC04_4_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74AHC04_5_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "11")
        )
      )
      (symbol "74AHC04_6_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74AHC04_7_0"
        (pin power_in line (at -1.27 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at -1.27 -7.62 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74AHC04_7_1"
        (rectangle (start -5.08 7.62) (end 2.54 -2.54)
          (fill (type background))
        )
      )
    )
    (symbol "Conn_01x08_1" (pin_numbers hide) (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J4" (at 2.54 1.905 0))
      (property "Value" "Module" (at 2.54 10.16 0))
      (property "Footprint" "" (at 0 2.54 0))
      (property "Datasheet" "~" (at 0 2.54 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (at 0 0 0))
      (symbol "Conn_01x08_1_1_1"
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 7.747) (end 0 7.493)
          (fill (type none))
        )
        (rectangle (start -1.27 8.89) (end 13.97 -1.27)
          (fill (type background))
        )
        (rectangle (start 13.97 -0.127) (end 12.7 0.127)
          (fill (type none))
        )
        (rectangle (start 13.97 2.413) (end 12.7 2.667)
          (fill (type none))
        )
        (rectangle (start 13.97 4.953) (end 12.7 5.207)
          (fill (type none))
        )
        (rectangle (start 13.97 7.493) (end 12.7 7.747)
          (fill (type none))
        )
        (pin passive line (at 17.78 2.54 180) (length 3.81)
          (name "+3V3")
          (number "1")
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "SC")
          (number "2")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "SD")
          (number "3")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "ULS")
          (number "4")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "LLS")
          (number "5")
        )
        (pin passive line (at 17.78 5.08 180) (length 3.81)
          (name "MOTOR2")
          (number "6")
        )
        (pin passive line (at 17.78 7.62 180) (length 3.81)
          (name "MOTOR1")
          (number "7")
        )
        (pin passive line (at 17.78 0 180) (length 3.81)
          (name "GND")
          (number "8")
        )
      )
    )
    (symbol "Connector_Generic:Conn_01x04" (pin_numbers hide) (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J8" (at -3.81 1.27 90))
      (property "Value" "Button Panel" (at -1.27 -7.62 90))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (at 0 0 0))
      (symbol "Conn_01x04_1_1"
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 3.81) (end 6.35 -6.35)
          (fill (type background))
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "+3V3")
          (number "1")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "GND")
          (number "2")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "UP")
          (number "3")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "DOWN")
          (number "4")
        )
      )
    )
    (symbol "Connector_Generic:Conn_01x16" (pin_numbers hide) (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J1" (at -12.7 -22.86 0))
      (property "Value" "Motor Driver" (at 2.54 -22.86 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x16, script generated (kicad-library-utils/schlib/autogen/connector/)" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (at 0 0 0))
      (symbol "Conn_01x16_1_1"
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 7.747) (end 0 7.493)
          (fill (type none))
        )
        (rectangle (start -1.27 10.287) (end 0 10.033)
          (fill (type none))
        )
        (rectangle (start -1.27 12.827) (end 0 12.573)
          (fill (type none))
        )
        (rectangle (start -1.27 15.367) (end 0 15.113)
          (fill (type none))
        )
        (rectangle (start -1.27 17.907) (end 0 17.653)
          (fill (type none))
        )
        (rectangle (start -1.27 19.05) (end 13.97 -6.35)
          (fill (type background))
        )
        (rectangle (start 13.97 4.953) (end 12.7 5.207)
          (fill (type none))
        )
        (rectangle (start 13.97 7.493) (end 12.7 7.747)
          (fill (type none))
        )
        (rectangle (start 13.97 10.033) (end 12.7 10.287)
          (fill (type none))
        )
        (rectangle (start 13.97 12.573) (end 12.7 12.827)
          (fill (type none))
        )
        (rectangle (start 13.97 15.113) (end 12.7 15.367)
          (fill (type none))
        )
        (rectangle (start 13.97 17.653) (end 12.7 17.907)
          (fill (type none))
        )
        (pin passive line (at -5.08 17.78 0) (length 3.81)
          (name "PWMB")
          (number "1")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "M+")
          (number "10")
        )
        (pin passive line (at 17.78 5.08 180) (length 3.81)
          (name "PS+")
          (number "11")
        )
        (pin passive line (at 17.78 7.62 180) (length 3.81)
          (name "PS-")
          (number "12")
        )
        (pin passive line (at 17.78 10.16 180) (length 3.81)
          (name "GND")
          (number "13")
        )
        (pin passive line (at 17.78 12.7 180) (length 3.81)
          (name "GND")
          (number "14")
        )
        (pin passive line (at 17.78 15.24 180) (length 3.81)
          (name "+3V3")
          (number "15")
        )
        (pin passive line (at 17.78 17.78 180) (length 3.81)
          (name "+3V3")
          (number "16")
        )
        (pin passive line (at -5.08 15.24 0) (length 3.81)
          (name "INB2")
          (number "2")
        )
        (pin passive line (at -5.08 12.7 0) (length 3.81)
          (name "INB1")
          (number "3")
        )
        (pin passive line (at -5.08 10.16 0) (length 3.81)
          (name "PWMA")
          (number "4")
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "INA2")
          (number "5")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "INA1")
          (number "6")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "M-")
          (number "7")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "M+")
          (number "8")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "M-")
          (number "9")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x02_Counter_Clockwise" (pin_numbers hide) (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J9" (at -0.635 7.62 0))
      (property "Value" "Power Distribution Board" (at -0.635 5.08 0))
      (property "Footprint" "" (at -8.89 2.54 0))
      (property "Datasheet" "~" (at -8.89 2.54 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x02, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (at 0 0 0))
      (symbol "Conn_02x02_Counter_Clockwise_1_1"
        (rectangle (start -10.16 0.127) (end -8.89 -0.127)
          (fill (type none))
        )
        (rectangle (start -10.16 2.667) (end -8.89 2.413)
          (fill (type none))
        )
        (rectangle (start -10.16 3.81) (end 8.89 -3.81)
          (fill (type background))
        )
        (rectangle (start 7.62 -2.413) (end 8.89 -2.667)
          (fill (type none))
        )
        (rectangle (start 7.62 0.127) (end 8.89 -0.127)
          (fill (type none))
        )
        (rectangle (start 7.62 2.667) (end 8.89 2.413)
          (fill (type none))
        )
        (pin power_in line (at -13.97 2.54 0) (length 3.81)
          (name "+15V_IN")
          (number "1")
        )
        (pin power_in line (at -13.97 0 0) (length 3.81)
          (name "GND")
          (number "2")
        )
        (pin passive line (at 12.7 -2.54 180) (length 3.81)
          (name "+3V3_OUT")
          (number "3")
        )
        (pin passive line (at 12.7 0 180) (length 3.81)
          (name "GND")
          (number "4")
        )
        (pin passive line (at 12.7 2.54 180) (length 3.81)
          (name "+5V_OUT")
          (number "5")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x11_Odd_Even" (pin_numbers hide) (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J3" (at 1.27 17.78 0))
      (property "Value" "MCU" (at 1.27 15.24 0))
      (property "Footprint" "" (at 0 5.08 0))
      (property "Datasheet" "~" (at 0 5.08 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x11, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (at 0 0 0))
      (symbol "Conn_02x11_Odd_Even_1_1"
        (rectangle (start -1.27 -7.493) (end 0 -7.747)
          (fill (type none))
        )
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 7.747) (end 0 7.493)
          (fill (type none))
        )
        (rectangle (start -1.27 10.287) (end 0 10.033)
          (fill (type none))
        )
        (rectangle (start -1.27 12.827) (end 0 12.573)
          (fill (type none))
        )
        (rectangle (start -1.27 13.97) (end 13.97 -8.89)
          (fill (type background))
        )
        (rectangle (start 4.953 -8.89) (end 5.207 -7.62)
          (fill (type none))
        )
        (rectangle (start 5.207 13.97) (end 4.953 12.7)
          (fill (type none))
        )
        (rectangle (start 7.493 -7.62) (end 7.747 -8.89)
          (fill (type none))
        )
        (rectangle (start 7.747 13.97) (end 7.493 12.7)
          (fill (type none))
        )
        (rectangle (start 13.97 -7.747) (end 12.7 -7.493)
          (fill (type none))
        )
        (rectangle (start 13.97 -4.953) (end 12.7 -5.207)
          (fill (type none))
        )
        (rectangle (start 13.97 -2.413) (end 12.7 -2.667)
          (fill (type none))
        )
        (rectangle (start 13.97 0.127) (end 12.7 -0.127)
          (fill (type none))
        )
        (rectangle (start 13.97 2.667) (end 12.7 2.413)
          (fill (type none))
        )
        (rectangle (start 13.97 5.207) (end 12.7 4.953)
          (fill (type none))
        )
        (rectangle (start 13.97 7.747) (end 12.7 7.493)
          (fill (type none))
        )
        (rectangle (start 13.97 10.287) (end 12.7 10.033)
          (fill (type none))
        )
        (rectangle (start 13.97 12.827) (end 12.7 12.573)
          (fill (type none))
        )
        (pin passive line (at -5.08 12.7 0) (length 3.81)
          (name "+5V")
          (number "1")
        )
        (pin passive line (at 17.78 2.54 180) (length 3.81)
          (name "IO")
          (number "10")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "IO")
          (number "11")
        )
        (pin passive line (at 17.78 0 180) (length 3.81)
          (name "IO")
          (number "12")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "IO")
          (number "13")
        )
        (pin passive line (at 17.78 -2.54 180) (length 3.81)
          (name "IO")
          (number "14")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "IO")
          (number "15")
        )
        (pin passive line (at 17.78 -5.08 180) (length 3.81)
          (name "IO")
          (number "16")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "IO")
          (number "17")
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "IO")
          (number "19")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "IO")
          (number "19")
        )
        (pin passive line (at 17.78 -7.62 180) (length 3.81)
          (name "IO")
          (number "19")
        )
        (pin passive line (at 17.78 12.7 180) (length 3.81)
          (name "IO")
          (number "2")
        )
        (pin passive line (at 5.08 -12.7 90) (length 3.81)
          (name "IO")
          (number "21")
        )
        (pin passive line (at 7.62 -12.7 90) (length 3.81)
          (name "IO")
          (number "22")
        )
        (pin passive line (at -5.08 10.16 0) (length 3.81)
          (name "GND")
          (number "3")
        )
        (pin passive line (at 17.78 10.16 180) (length 3.81)
          (name "IO")
          (number "4")
        )
        (pin passive line (at 5.08 17.78 270) (length 3.81)
          (name "SDA")
          (number "5")
        )
        (pin passive line (at 17.78 7.62 180) (length 3.81)
          (name "IO")
          (number "6")
        )
        (pin passive line (at 7.62 17.78 270) (length 3.81)
          (name "SCL")
          (number "7")
        )
        (pin passive line (at 17.78 5.08 180) (length 3.81)
          (name "IO")
          (number "8")
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "IO")
          (number "9")
        )
      )
    )
    (symbol "Interface_Expansion:PCA9544AD" (pin_numbers hide) (in_bom yes) (on_board yes)
      (property "Reference" "U2" (at 24.13 -1.9559 0))
      (property "Value" "I2C Multiplexer" (at -13.97 -12.7 90))
      (property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (at -21.59 -25.4 0))
      (property "Datasheet" "http://www.nxp.com/documents/data_sheet/PCA9544A.pdf" (at -27.94 5.08 0))
      (property "ki_keywords" "i2c multiplexer" (at 0 0 0))
      (property "ki_description" "4-channel I2C-bus multiplexer with interrupt logic, SOIC-20" (at 0 0 0))
      (property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*" (at 0 0 0))
      (symbol "PCA9544AD_0_1"
        (rectangle (start -2.54 20.32) (end 10.16 -20.32)
          (fill (type background))
        )
      )
      (symbol "PCA9544AD_1_1"
        (pin power_in line (at 3.81 -22.86 90) (length 2.54)
          (name "VIN")
          (number "10")
        )
        (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
          (name "SD2")
          (number "12")
        )
        (pin output line (at 12.7 -5.08 180) (length 2.54)
          (name "SC2")
          (number "13")
        )
        (pin bidirectional line (at 12.7 -12.7 180) (length 2.54)
          (name "SD3")
          (number "15")
        )
        (pin output line (at 12.7 -15.24 180) (length 2.54)
          (name "SC3")
          (number "16")
        )
        (pin input line (at -5.08 -1.27 0) (length 2.54)
          (name "SCL")
          (number "18")
        )
        (pin bidirectional line (at -5.08 1.27 0) (length 2.54)
          (name "SDA")
          (number "19")
        )
        (pin power_in line (at 3.81 22.86 270) (length 2.54)
          (name "GND")
          (number "20")
        )
        (pin bidirectional line (at 12.7 17.78 180) (length 2.54)
          (name "SD0")
          (number "5")
        )
        (pin output line (at 12.7 15.24 180) (length 2.54)
          (name "SC0")
          (number "6")
        )
        (pin bidirectional line (at 12.7 7.62 180) (length 2.54)
          (name "SD1")
          (number "8")
        )
        (pin output line (at 12.7 5.08 180) (length 2.54)
          (name "SC1")
          (number "9")
        )
      )
    )
    (symbol "power:+15V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+15V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+15V\"" (at 0 0 0))
      (symbol "+15V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+15V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+15V")
          (number "1")
        )
      )
    )
    (symbol "power:+3V3" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+3V3" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3V3\"" (at 0 0 0))
      (symbol "+3V3_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3V3_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+5V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 123.19 102.87) (diameter 0) (color 0 0 0 0))
  (junction (at 123.19 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 123.19 73.66) (diameter 0) (color 0 0 0 0))
  (junction (at 123.19 113.03) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 102.87 81.28) (xy 123.19 81.28)))
  (wire (pts (xy 102.87 86.36) (xy 106.68 86.36)))
  (wire (pts (xy 147.32 107.95) (xy 147.32 113.03)))
  (wire (pts (xy 132.08 97.79) (xy 137.16 97.79)))
  (wire (pts (xy 160.02 82.55) (xy 165.1 82.55)))
  (wire (pts (xy 147.32 72.39) (xy 147.32 77.47)))
  (wire (pts (xy 102.87 110.49) (xy 123.19 110.49)))
  (wire (pts (xy 123.19 113.03) (xy 127 113.03)))
  (wire (pts (xy 132.08 100.33) (xy 137.16 100.33)))
  (wire (pts (xy 102.87 115.57) (xy 106.68 115.57)))
  (wire (pts (xy 102.87 107.95) (xy 106.68 107.95)))
  (wire (pts (xy 132.08 95.25) (xy 137.16 95.25)))
  (wire (pts (xy 102.87 105.41) (xy 123.19 105.41)))
  (wire (pts (xy 123.19 81.28) (xy 123.19 83.82)))
  (wire (pts (xy 102.87 76.2) (xy 123.19 76.2)))
  (wire (pts (xy 149.86 107.95) (xy 149.86 113.03)))
  (wire (pts (xy 132.08 87.63) (xy 137.16 87.63)))
  (wire (pts (xy 123.19 102.87) (xy 127 102.87)))
  (wire (pts (xy 132.08 92.71) (xy 137.16 92.71)))
  (wire (pts (xy 123.19 73.66) (xy 127 73.66)))
  (wire (pts (xy 123.19 83.82) (xy 127 83.82)))
  (wire (pts (xy 123.19 105.41) (xy 123.19 102.87)))
  (wire (pts (xy 123.19 110.49) (xy 123.19 113.03)))
  (wire (pts (xy 102.87 83.82) (xy 113.03 83.82)))
  (wire (pts (xy 113.03 102.87) (xy 102.87 102.87)))
  (wire (pts (xy 102.87 113.03) (xy 113.03 113.03)))
  (wire (pts (xy 113.03 73.66) (xy 102.87 73.66)))
  (wire (pts (xy 123.19 76.2) (xy 123.19 73.66)))
  (wire (pts (xy 132.08 102.87) (xy 137.16 102.87)))
  (wire (pts (xy 132.08 90.17) (xy 137.16 90.17)))
  (wire (pts (xy 102.87 78.74) (xy 106.68 78.74)))
  (wire (pts (xy 149.86 72.39) (xy 149.86 77.47)))
  (label "IO6" (at 106.68 107.95 180) (fields_autoplaced))
  (label "IO8" (at 106.68 115.57 180) (fields_autoplaced))
  (label "IO5" (at 127 102.87 180) (fields_autoplaced))
  (label "IO7" (at 132.08 102.87 0) (fields_autoplaced))
  (label "IO3" (at 127 83.82 180) (fields_autoplaced))
  (label "IO5" (at 132.08 97.79 0) (fields_autoplaced))
  (label "IO4" (at 106.68 86.36 180) (fields_autoplaced))
  (label "IO6" (at 132.08 100.33 0) (fields_autoplaced))
  (label "IO2" (at 132.08 90.17 0) (fields_autoplaced))
  (label "IO7" (at 127 113.03 180) (fields_autoplaced))
  (label "IO4" (at 132.08 95.25 0) (fields_autoplaced))
  (label "IO2" (at 106.68 78.74 180) (fields_autoplaced))
  (label "IO1" (at 132.08 87.63 0) (fields_autoplaced))
  (label "IO1" (at 127 73.66 180) (fields_autoplaced))
  (label "IO8" (at 165.1 82.55 180) (fields_autoplaced))
  (label "IO3" (at 132.08 92.71 0) (fields_autoplaced))
  (global_label "MOTORC2" (shape input) (at 200.66 99.06 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 212.3953 99.06 0))
  )
  (global_label "SD2" (shape input) (at 177.8 99.06 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 171.2052 99.06 0))
  )
  (global_label "MOTORC1" (shape input) (at 200.66 96.52 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 212.3953 96.52 0))
  )
  (global_label "SC0" (shape input) (at 177.8 68.58 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 171.2052 68.58 0))
  )
  (global_label "MOTORD1" (shape input) (at 102.87 97.79 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 114.6053 97.79 0))
  )
  (global_label "LLS4" (shape input) (at 177.8 118.11 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 170.419 118.11 0))
  )
  (global_label "SD0" (shape input) (at 177.8 71.12 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 171.2052 71.12 0))
  )
  (global_label "MOTORA1" (shape input) (at 200.66 68.58 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 212.2139 68.58 0))
  )
  (global_label "MOTORC2" (shape input) (at 102.87 95.25 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 114.6053 95.25 0))
  )
  (global_label "SD3" (shape input) (at 177.8 113.03 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 171.2052 113.03 0))
  )
  (global_label "MOTORA1" (shape input) (at 102.87 63.5 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 114.4239 63.5 0))
  )
  (global_label "MOTORD2" (shape input) (at 102.87 100.33 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 114.6053 100.33 0))
  )
  (global_label "SC2" (shape input) (at 177.8 96.52 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 171.2052 96.52 0))
  )
  (global_label "SC3" (shape input) (at 177.8 110.49 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 171.2052 110.49 0))
  )
  (global_label "LLS3" (shape input) (at 160.02 97.79 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 167.401 97.79 0))
  )
  (global_label "LLS2" (shape input) (at 177.8 90.17 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 170.419 90.17 0))
  )
  (global_label "SC3" (shape input) (at 163.83 54.61 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 163.83 48.0152 90))
  )
  (global_label "SD3" (shape input) (at 161.29 54.61 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 161.29 48.0152 90))
  )
  (global_label "SC2" (shape input) (at 153.67 54.61 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 153.67 48.0152 90))
  )
  (global_label "ULS3" (shape input) (at 160.02 95.25 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 167.7034 95.25 0))
  )
  (global_label "SC1" (shape input) (at 143.51 54.61 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 143.51 48.0152 90))
  )
  (global_label "SD1" (shape input) (at 177.8 85.09 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 171.2052 85.09 0))
  )
  (global_label "ULS1" (shape input) (at 177.8 73.66 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 170.1166 73.66 0))
  )
  (global_label "ULS3" (shape input) (at 177.8 101.6 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 170.1166 101.6 0))
  )
  (global_label "LLS3" (shape input) (at 177.8 104.14 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 170.419 104.14 0))
  )
  (global_label "ULS1" (shape input) (at 160.02 85.09 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 167.7034 85.09 0))
  )
  (global_label "MOTORD1" (shape input) (at 200.66 110.49 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 212.3953 110.49 0))
  )
  (global_label "MOTORA2" (shape input) (at 102.87 66.04 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 114.4239 66.04 0))
  )
  (global_label "MOTORB1" (shape input) (at 200.66 82.55 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 212.3953 82.55 0))
  )
  (global_label "MOTORB1" (shape input) (at 102.87 68.58 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 114.6053 68.58 0))
  )
  (global_label "ULS2" (shape input) (at 177.8 87.63 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 170.1166 87.63 0))
  )
  (global_label "MOTORB2" (shape input) (at 200.66 85.09 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 212.3953 85.09 0))
  )
  (global_label "LLS1" (shape input) (at 177.8 76.2 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 170.419 76.2 0))
  )
  (global_label "ULS2" (shape input) (at 160.02 90.17 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 167.7034 90.17 0))
  )
  (global_label "SC1" (shape input) (at 177.8 82.55 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 171.2052 82.55 0))
  )
  (global_label "LLS2" (shape input) (at 160.02 92.71 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 167.401 92.71 0))
  )
  (global_label "MOTORD2" (shape input) (at 200.66 113.03 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 212.3953 113.03 0))
  )
  (global_label "MOTORA2" (shape input) (at 200.66 71.12 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 212.2139 71.12 0))
  )
  (global_label "MOTORC1" (shape input) (at 102.87 92.71 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 114.6053 92.71 0))
  )
  (global_label "ULS4" (shape input) (at 160.02 100.33 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 167.7034 100.33 0))
  )
  (global_label "SD0" (shape input) (at 130.81 54.61 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 130.81 48.0152 90))
  )
  (global_label "SD1" (shape input) (at 140.97 54.61 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 140.97 48.0152 90))
  )
  (global_label "LLS4" (shape input) (at 160.02 102.87 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 167.401 102.87 0))
  )
  (global_label "MOTORB2" (shape input) (at 102.87 71.12 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 114.6053 71.12 0))
  )
  (global_label "ULS4" (shape input) (at 177.8 115.57 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 170.1166 115.57 0))
  )
  (global_label "LLS1" (shape input) (at 160.02 87.63 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 167.401 87.63 0))
  )
  (global_label "SD2" (shape input) (at 151.13 54.61 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 151.13 48.0152 90))
  )
  (global_label "SC0" (shape input) (at 133.35 54.61 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 133.35 48.0152 90))
  )
  (symbol (lib_name "Conn_01x08_1") (lib_id "Connector_Generic:Conn_01x08") (at 182.88 118.11 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J6" (at 185.42 116.205 0))
    (property "Value" "Module" (at 185.42 107.95 0))
    (property "Footprint" "" (at 182.88 115.57 0))
    (property "Datasheet" "~" (at 182.88 115.57 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "Main"
        (path
          (reference "J6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 137.16 85.09 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR016" (at 130.81 85.09 0))
    (property "Value" "GND" (at 134.62 85.09 90))
    (property "Footprint" "" (at 137.16 85.09 0))
    (property "Datasheet" "" (at 137.16 85.09 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR016") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 154.94 113.03 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR028" (at 154.94 116.84 0))
    (property "Value" "+3V3" (at 154.94 110.49 90))
    (property "Footprint" "" (at 154.94 113.03 0))
    (property "Datasheet" "" (at 154.94 113.03 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR028") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+15V") (at 104.14 50.8 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR032" (at 100.33 50.8 0))
    (property "Value" "+5V" (at 109.22 50.8 90))
    (property "Footprint" "" (at 104.14 50.8 0))
    (property "Datasheet" "" (at 104.14 50.8 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR032") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 80.01 76.2 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR03" (at 73.66 76.2 0))
    (property "Value" "GND" (at 77.47 76.2 90))
    (property "Footprint" "" (at 80.01 76.2 0))
    (property "Datasheet" "" (at 80.01 76.2 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector_Generic:Conn_01x04") (at 152.4 118.11 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J8" (at 153.67 114.3 90))
    (property "Value" "Button Panel" (at 151.13 125.73 90))
    (property "Footprint" "" (at 152.4 118.11 0))
    (property "Datasheet" "~" (at 152.4 118.11 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (instances
      (project "Main"
        (path
          (reference "J8") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "74xx:74AHC04") (at 119.38 83.82 180) (unit 2)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U1" (at 127 83.82 0))
    (property "Value" "74AHC04" (at 119.38 86.36 0))
    (property "Footprint" "" (at 119.38 83.82 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT04.pdf" (at 128.27 83.82 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "Main"
        (path
          (reference "U1") (unit 2)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 128.27 123.19 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR014" (at 134.62 123.19 0))
    (property "Value" "GND" (at 130.81 123.19 90))
    (property "Footprint" "" (at 128.27 123.19 0))
    (property "Datasheet" "" (at 128.27 123.19 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR014") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 107.95 123.19 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR013" (at 111.76 123.19 0))
    (property "Value" "+3V3" (at 105.41 123.19 90))
    (property "Footprint" "" (at 107.95 123.19 0))
    (property "Datasheet" "" (at 107.95 123.19 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR013") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+15V") (at 171.45 63.5 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR08" (at 167.64 63.5 0))
    (property "Value" "+3V3" (at 176.53 63.5 90))
    (property "Footprint" "" (at 171.45 63.5 0))
    (property "Datasheet" "" (at 171.45 63.5 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR08") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 104.14 53.34 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR031" (at 110.49 53.34 0))
    (property "Value" "GND" (at 106.68 53.34 90))
    (property "Footprint" "" (at 104.14 53.34 0))
    (property "Datasheet" "" (at 104.14 53.34 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR031") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 200.66 115.57 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR017" (at 196.85 115.57 0))
    (property "Value" "+3V3" (at 203.2 115.57 90))
    (property "Footprint" "" (at 200.66 115.57 0))
    (property "Datasheet" "" (at 200.66 115.57 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR017") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 200.66 104.14 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR012" (at 207.01 104.14 0))
    (property "Value" "GND" (at 203.2 104.14 90))
    (property "Footprint" "" (at 200.66 104.14 0))
    (property "Datasheet" "" (at 200.66 104.14 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR012") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+15V") (at 104.14 55.88 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR033" (at 100.33 55.88 0))
    (property "Value" "+3V3" (at 109.22 55.88 90))
    (property "Footprint" "" (at 104.14 55.88 0))
    (property "Datasheet" "" (at 104.14 55.88 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR033") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 137.16 82.55 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR015" (at 140.97 82.55 0))
    (property "Value" "+5V" (at 134.62 82.55 90))
    (property "Footprint" "" (at 137.16 82.55 0))
    (property "Datasheet" "" (at 137.16 82.55 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR015") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 80.01 86.36 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR02" (at 83.82 86.36 0))
    (property "Value" "+3V3" (at 77.47 86.36 90))
    (property "Footprint" "" (at 80.01 86.36 0))
    (property "Datasheet" "" (at 80.01 86.36 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector_Generic:Conn_02x02_Counter_Clockwise") (at 91.44 53.34 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "J9" (at 90.805 45.72 0))
    (property "Value" "Power Distribution Board" (at 90.805 48.26 0))
    (property "Footprint" "" (at 82.55 50.8 0))
    (property "Datasheet" "~" (at 82.55 50.8 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (instances
      (project "Main"
        (path
          (reference "J9") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 200.66 90.17 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR010" (at 207.01 90.17 0))
    (property "Value" "GND" (at 203.2 90.17 90))
    (property "Footprint" "" (at 200.66 90.17 0))
    (property "Datasheet" "" (at 200.66 90.17 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR010") (unit 1)
        )
      )
    )
  )
  (symbol (lib_name "74AHC04_1") (lib_id "74xx:74AHC04") (at 120.65 121.92 90) (unit 7)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U1" (at 120.65 129.54 0))
    (property "Value" "74AHC04" (at 118.11 118.11 90))
    (property "Footprint" "" (at 120.65 121.92 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT04.pdf" (at 120.65 130.81 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "Main"
        (path
          (reference "U1") (unit 7)
        )
      )
    )
  )
  (symbol (lib_id "Connector_Generic:Conn_02x11_Odd_Even") (at 142.24 95.25 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J3" (at 143.51 77.47 0))
    (property "Value" "MCU" (at 143.51 80.01 0))
    (property "Footprint" "" (at 142.24 90.17 0))
    (property "Datasheet" "~" (at 142.24 90.17 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "19")
    (pin "19")
    (pin "19")
    (pin "2")
    (pin "21")
    (pin "22")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "Main"
        (path
          (reference "J3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+15V") (at 80.01 102.87 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR034" (at 83.82 102.87 0))
    (property "Value" "+15V_PS" (at 77.47 102.87 90))
    (property "Footprint" "" (at 80.01 102.87 0))
    (property "Datasheet" "" (at 80.01 102.87 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR034") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 80.01 115.57 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR039" (at 83.82 115.57 0))
    (property "Value" "+3V3" (at 77.47 115.57 90))
    (property "Footprint" "" (at 80.01 115.57 0))
    (property "Datasheet" "" (at 80.01 115.57 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR039") (unit 1)
        )
      )
    )
  )
  (symbol (lib_name "Conn_01x08_1") (lib_id "Connector_Generic:Conn_01x08") (at 182.88 90.17 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J2" (at 185.42 88.265 0))
    (property "Value" "Module" (at 185.42 80.01 0))
    (property "Footprint" "" (at 182.88 87.63 0))
    (property "Datasheet" "~" (at 182.88 87.63 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "Main"
        (path
          (reference "J2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+15V") (at 80.01 73.66 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR05" (at 83.82 73.66 0))
    (property "Value" "+15V_PS" (at 77.47 73.66 90))
    (property "Footprint" "" (at 80.01 73.66 0))
    (property "Datasheet" "" (at 80.01 73.66 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR05") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 80.01 83.82 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR01" (at 83.82 83.82 0))
    (property "Value" "+3V3" (at 77.47 83.82 90))
    (property "Footprint" "" (at 80.01 83.82 0))
    (property "Datasheet" "" (at 80.01 83.82 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 200.66 76.2 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR020" (at 207.01 76.2 0))
    (property "Value" "GND" (at 203.2 76.2 90))
    (property "Footprint" "" (at 200.66 76.2 0))
    (property "Datasheet" "" (at 200.66 76.2 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR020") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 80.01 78.74 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR04" (at 73.66 78.74 0))
    (property "Value" "GND" (at 77.47 78.74 90))
    (property "Footprint" "" (at 80.01 78.74 0))
    (property "Datasheet" "" (at 80.01 78.74 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
    )
  )
  (symbol (lib_name "Conn_01x08_1") (lib_id "Connector_Generic:Conn_01x08") (at 182.88 104.14 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J5" (at 185.42 102.235 0))
    (property "Value" "Module" (at 185.42 93.98 0))
    (property "Footprint" "" (at 182.88 101.6 0))
    (property "Datasheet" "~" (at 182.88 101.6 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "Main"
        (path
          (reference "J5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 80.01 81.28 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR06" (at 73.66 81.28 0))
    (property "Value" "GND" (at 77.47 81.28 90))
    (property "Footprint" "" (at 80.01 81.28 0))
    (property "Datasheet" "" (at 80.01 81.28 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR06") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector_Generic:Conn_01x16") (at 97.79 97.79 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J10" (at 110.49 74.93 0))
    (property "Value" "Motor Driver" (at 91.44 90.17 0))
    (property "Footprint" "" (at 97.79 97.79 0))
    (property "Datasheet" "~" (at 97.79 97.79 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "Main"
        (path
          (reference "J10") (unit 1)
        )
      )
    )
  )
  (symbol (lib_name "74AHC04_3") (lib_id "74xx:74AHC04") (at 119.38 113.03 180) (unit 2)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U3" (at 119.38 107.95 0))
    (property "Value" "74AHC04" (at 119.38 115.57 0))
    (property "Footprint" "" (at 119.38 113.03 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT04.pdf" (at 119.38 104.14 0))
    (pin "1")
    (pin "2")
    (pin "7")
    (pin "8")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "Main"
        (path
          (reference "U3") (unit 2)
        )
      )
    )
  )
  (symbol (lib_name "Conn_01x08_1") (lib_id "Connector_Generic:Conn_01x08") (at 182.88 76.2 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J4" (at 185.42 74.295 0))
    (property "Value" "Module" (at 185.42 66.04 0))
    (property "Footprint" "" (at 182.88 73.66 0))
    (property "Datasheet" "~" (at 182.88 73.66 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "Main"
        (path
          (reference "J4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_name "74AHC04_4") (lib_id "74xx:74AHC04") (at 119.38 73.66 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U1" (at 127 73.66 0))
    (property "Value" "74AHC04" (at 119.38 71.12 0))
    (property "Footprint" "" (at 119.38 73.66 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT04.pdf" (at 128.27 73.66 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "Main"
        (path
          (reference "U1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 200.66 118.11 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR018" (at 207.01 118.11 0))
    (property "Value" "GND" (at 203.2 118.11 90))
    (property "Footprint" "" (at 200.66 118.11 0))
    (property "Datasheet" "" (at 200.66 118.11 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR018") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 200.66 73.66 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR019" (at 196.85 73.66 0))
    (property "Value" "+3V3" (at 203.2 73.66 90))
    (property "Footprint" "" (at 200.66 73.66 0))
    (property "Datasheet" "" (at 200.66 73.66 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR019") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+15V") (at 77.47 50.8 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR029" (at 81.28 50.8 0))
    (property "Value" "+15V_PS" (at 69.85 50.8 90))
    (property "Footprint" "" (at 77.47 50.8 0))
    (property "Datasheet" "" (at 77.47 50.8 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR029") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 80.01 105.41 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR035" (at 73.66 105.41 0))
    (property "Value" "GND" (at 77.47 105.41 90))
    (property "Footprint" "" (at 80.01 105.41 0))
    (property "Datasheet" "" (at 80.01 105.41 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR035") (unit 1)
        )
      )
    )
  )
  (symbol (lib_name "74AHC04_2") (lib_id "74xx:74AHC04") (at 119.38 102.87 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U1C" (at 119.38 107.95 0))
    (property "Value" "74AHC04" (at 119.38 100.33 0))
    (property "Footprint" "" (at 119.38 102.87 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74AHC_AHCT04.pdf" (at 119.38 93.98 0))
    (pin "5")
    (pin "6")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "Main"
        (path
          (reference "U1C") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 200.66 87.63 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR09" (at 196.85 87.63 0))
    (property "Value" "+3V3" (at 203.2 87.63 90))
    (property "Footprint" "" (at 200.66 87.63 0))
    (property "Datasheet" "" (at 200.66 87.63 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR09") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 200.66 101.6 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR011" (at 196.85 101.6 0))
    (property "Value" "+3V3" (at 203.2 101.6 90))
    (property "Footprint" "" (at 200.66 101.6 0))
    (property "Datasheet" "" (at 200.66 101.6 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR011") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 80.01 110.49 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR037" (at 73.66 110.49 0))
    (property "Value" "GND" (at 77.47 110.49 90))
    (property "Footprint" "" (at 80.01 110.49 0))
    (property "Datasheet" "" (at 80.01 110.49 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR037") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector_Generic:Conn_01x16") (at 97.79 68.58 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J1" (at 110.49 45.72 0))
    (property "Value" "Motor Driver" (at 91.44 60.96 0))
    (property "Footprint" "" (at 97.79 68.58 0))
    (property "Datasheet" "~" (at 97.79 68.58 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "Main"
        (path
          (reference "J1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Interface_Expansion:PCA9544AD") (at 148.59 67.31 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U2" (at 150.5459 43.18 0))
    (property "Value" "I2C Multiplexer" (at 162.56 71.12 90))
    (property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (at 173.99 88.9 0))
    (property "Datasheet" "http://www.nxp.com/documents/data_sheet/PCA9544A.pdf" (at 143.51 95.25 0))
    (pin "10")
    (pin "12")
    (pin "13")
    (pin "15")
    (pin "16")
    (pin "18")
    (pin "19")
    (pin "20")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (instances
      (project "Main"
        (path
          (reference "U2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 125.73 63.5 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR07" (at 119.38 63.5 0))
    (property "Value" "GND" (at 123.19 63.5 90))
    (property "Footprint" "" (at 125.73 63.5 0))
    (property "Datasheet" "" (at 125.73 63.5 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR07") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 77.47 53.34 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR030" (at 71.12 53.34 0))
    (property "Value" "GND" (at 74.93 53.34 90))
    (property "Footprint" "" (at 77.47 53.34 0))
    (property "Datasheet" "" (at 77.47 53.34 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR030") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+3V3") (at 80.01 113.03 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR038" (at 83.82 113.03 0))
    (property "Value" "+3V3" (at 77.47 113.03 90))
    (property "Footprint" "" (at 80.01 113.03 0))
    (property "Datasheet" "" (at 80.01 113.03 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR038") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 80.01 107.95 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR036" (at 73.66 107.95 0))
    (property "Value" "GND" (at 77.47 107.95 90))
    (property "Footprint" "" (at 80.01 107.95 0))
    (property "Datasheet" "" (at 80.01 107.95 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR036") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 152.4 113.03 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR027" (at 152.4 106.68 0))
    (property "Value" "GND" (at 152.4 110.49 90))
    (property "Footprint" "" (at 152.4 113.03 0))
    (property "Datasheet" "" (at 152.4 113.03 0))
    (pin "1")
    (instances
      (project "Main"
        (path
          (reference "#PWR027") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
