(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plots/")
    )
  )
  (net 0 "")
  (net 1 "Net-(J4-Pin_1)")
  (net 2 "/MOTOR_POS")
  (net 3 "/ULS")
  (net 4 "GND")
  (net 5 "/LLS")
  (net 6 "+3V3")
  (net 7 "/SDA")
  (net 8 "/SCL")
  (net 9 "/MOTOR_NEG")
  (footprint "" (layer "F.Cu")
    (at 113.411 63.246)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 134.62 63.246 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Module Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.82 90) (layer "F.SilkS") hide)
    (fp_text value "1k" (at 0 1.82 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 3 "/ULS") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 6 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 137.16 63.22 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Module Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.82 90) (layer "F.SilkS") hide)
    (fp_text value "1k" (at 0 1.82 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 5 "/LLS") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 6 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MOLEX_1053131302:1053131302" (layer "F.Cu")
    (at 127.2915 64.711001 180)
    (property "Sheetfile" "Module Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -2.2485 -5.669999) (layer "F.SilkS") hide)
    (fp_text value "UPPER LS" (at 2.5775 4.640001 90) (layer "F.SilkS"))
    (fp_text user "MAXIMUM_PACKAGE_HEIGHT:_6.64_MM" (at -4.219994 20.000001) (layer "Cmts.User"))
    (fp_text user "MAXIMUM_PACKAGE_HEIGHT:_6.64_MM" (at -4.219994 20.000001) (layer "Cmts.User"))
    (fp_text user "NOTE" (at -4.219994 17.460001) (layer "Cmts.User"))
    (fp_text user "NOTE" (at -4.219994 17.460001) (layer "Cmts.User"))
    (fp_text user "1.6_MM_TO_2.4_MM" (at -4.219994 26.350001) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "RECOMMENDED_PCB_THICKNESS:" (at -4.219994 23.810001) (layer "Cmts.User"))
    (fp_text user "1.6_MM_TO_2.4_MM" (at -4.219994 26.350001) (layer "Cmts.User"))
    (fp_text user "RECOMMENDED_PCB_THICKNESS:" (at -4.219994 23.810001) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.499995 7.180001 180) (size 1.6 1.6) (drill 1.6) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 0 7.180001 180) (size 1.6 1.6) (drill 1.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 3 "/ULS") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.5 0 180) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/1053131302.stp"
      (offset (xyz -1.2 -6.1 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (layer "F.Cu")
    (at 113.411 57.785)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "B.Cu" "B.Mask"))
  )
  (footprint "MOLEX_1053141304:1053141304" (layer "F.Cu")
    (at 122.388 80.478 -90)
    (property "Sheetfile" "Module Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at -1.25 -6.35 90) (layer "F.SilkS") hide)
    (fp_text value "ENCODER" (at 3.088005 4.528001) (layer "F.SilkS"))
    (fp_text user "MAXIMUM_PACKAGE_HEIGHT:_9.14_MM" (at -4.219994 22.542002 90) (layer "Cmts.User"))
    (fp_text user "1.6_MM_TO_2.4_MM" (at -4.219994 28.892001 90) (layer "Cmts.User"))
    (fp_text user "RECOMMENDED_PCB_THICKNESS:" (at -4.219994 26.352001 90) (layer "Cmts.User"))
    (fp_text user "MAXIMUM_PACKAGE_HEIGHT:_9.14_MM" (at -4.219994 22.542002 90) (layer "Cmts.User"))
    (fp_text user "NOTE" (at -4.219994 20.002002 90) (layer "Cmts.User"))
    (fp_text user "1.6_MM_TO_2.4_MM" (at -4.219994 28.892001 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "NOTE" (at -4.219994 20.002002 90) (layer "Cmts.User"))
    (fp_text user "RECOMMENDED_PCB_THICKNESS:" (at -4.219994 26.352001 90) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.499995 9.680001 270) (size 1.6 1.6) (drill 1.6) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 0 9.680001 270) (size 1.6 1.6) (drill 1.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 7 "/SDA") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.5 0 270) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 8 "/SCL") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 2.5 270) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at -2.5 2.5 270) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 6 "+3V3") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KIPRJMOD}/1053141304.stp"
      (offset (xyz -1.25 -8.6 3.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 180))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (layer "F.Cu")
    (at 113.411 63.246)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "B.Cu" "B.Mask"))
  )
  (footprint "MOLEX_1053131302:1053131302" (layer "F.Cu")
    (at 118.785005 64.711001 180)
    (property "Sheetfile" "Module Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at -0.383488 -3.383999) (layer "F.SilkS") hide)
    (fp_text value "LOWER LS" (at 2.664512 4.640001 90) (layer "F.SilkS"))
    (fp_text user "NOTE" (at -4.219994 17.460001) (layer "Cmts.User"))
    (fp_text user "MAXIMUM_PACKAGE_HEIGHT:_6.64_MM" (at -4.219994 20.000001) (layer "Cmts.User"))
    (fp_text user "1.6_MM_TO_2.4_MM" (at -4.219994 26.350001) (layer "Cmts.User"))
    (fp_text user "RECOMMENDED_PCB_THICKNESS:" (at -4.219994 23.810001) (layer "Cmts.User"))
    (fp_text user "RECOMMENDED_PCB_THICKNESS:" (at -4.219994 23.810001) (layer "Cmts.User"))
    (fp_text user "1.6_MM_TO_2.4_MM" (at -4.219994 26.350001) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "NOTE" (at -4.219994 17.460001) (layer "Cmts.User"))
    (fp_text user "MAXIMUM_PACKAGE_HEIGHT:_6.64_MM" (at -4.219994 20.000001) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.499995 7.180001 180) (size 1.6 1.6) (drill 1.6) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 0 7.180001 180) (size 1.6 1.6) (drill 1.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 5 "/LLS") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.5 0 180) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/1053131302.stp"
      (offset (xyz -1.2 -6.1 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "MOLEX_1053141308:1053141308" (layer "F.Cu")
    (at 127.294 69.462015 90)
    (property "Sheetfile" "Module Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at -3.75 -6.35 90) (layer "F.SilkS") hide)
    (fp_text value "INPUT" (at 2.660015 3.008 180) (layer "F.SilkS"))
    (fp_text user "RECOMMENDED_PCB_THICKNESS:" (at -9.219989 26.352001 90) (layer "Cmts.User"))
    (fp_text user "1.6_MM_TO_2.4_MM" (at -9.219989 28.892001 90) (layer "Cmts.User"))
    (fp_text user "NOTE" (at -9.219989 20.002002 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "MAXIMUM_PACKAGE_HEIGHT:_9.14_MM" (at -9.219989 22.542002 90) (layer "Cmts.User"))
    (fp_text user "1.6_MM_TO_2.4_MM" (at -9.219989 28.892001 90) (layer "Cmts.User"))
    (fp_text user "NOTE" (at -9.219989 20.002002 90) (layer "Cmts.User"))
    (fp_text user "MAXIMUM_PACKAGE_HEIGHT:_9.14_MM" (at -9.219989 22.542002 90) (layer "Cmts.User"))
    (fp_text user "RECOMMENDED_PCB_THICKNESS:" (at -9.219989 26.352001 90) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -7.499985 9.680001 90) (size 1.6 1.6) (drill 1.6) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 0 9.680001 90) (size 1.6 1.6) (drill 1.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 9 "/MOTOR_NEG") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.5 0 90) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 2 "/MOTOR_POS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5 0 90) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 8 "/SCL") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at -7.5 0 90) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 7 "/SDA") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 2.5 90) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 3 "/ULS") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at -2.5 2.5 90) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 5 "/LLS") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at -5 2.5 90) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 6 "+3V3") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at -7.5 2.5 90) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KIPRJMOD}/1053141308.stp"
      (offset (xyz -3.75 -8.65 3.25))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "MOLEX_1053131302:1053131302" (layer "F.Cu")
    (at 119.891999 71.96 -90)
    (property "Sheetfile" "Module Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at -1.25 -6.35 90) (layer "F.SilkS") hide)
    (fp_text value "MOTOR" (at 2.97 3.556) (layer "F.SilkS"))
    (fp_text user "RECOMMENDED_PCB_THICKNESS:" (at -4.219994 23.810001 90) (layer "Cmts.User"))
    (fp_text user "MAXIMUM_PACKAGE_HEIGHT:_6.64_MM" (at -4.219994 20.000001 90) (layer "Cmts.User"))
    (fp_text user "MAXIMUM_PACKAGE_HEIGHT:_6.64_MM" (at -4.219994 20.000001 90) (layer "Cmts.User"))
    (fp_text user "NOTE" (at -4.219994 17.460001 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "RECOMMENDED_PCB_THICKNESS:" (at -4.219994 23.810001 90) (layer "Cmts.User"))
    (fp_text user "1.6_MM_TO_2.4_MM" (at -4.219994 26.350001 90) (layer "Cmts.User"))
    (fp_text user "NOTE" (at -4.219994 17.460001 90) (layer "Cmts.User"))
    (fp_text user "1.6_MM_TO_2.4_MM" (at -4.219994 26.350001 90) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.499995 7.180001 270) (size 1.6 1.6) (drill 1.6) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 0 7.180001 270) (size 1.6 1.6) (drill 1.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J4-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.5 0 270) (size 1.7 1.7) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 9 "/MOTOR_NEG") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/1053131302.stp"
      (offset (xyz -1.2 -6.1 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 123.6615 71.97)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "Module Board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Fuse")
    (property "ki_keywords" "fuse")
    (attr smd)
    (fp_text reference "F1" (at 0 -1.82) (layer "F.SilkS") hide)
    (fp_text value "10A" (at 0 1.82) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754392982)
      (net 1 "Net-(J4-Pin_1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1754392982)
      (net 2 "/MOTOR_POS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (layer "F.Cu")
    (at 136.144 57.785)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "B.Cu" "B.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (layer "F.Cu")
    (at 136.144 81.915)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad_TopBottom" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers "*.Cu" "*.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "F.Cu" "F.Mask"))
    (pad "1" connect circle (at 0 0) (size 3.8 3.8) (layers "B.Cu" "B.Mask"))
  )
  (footprint "Elevate_Logo:ElevateLogo" (layer "B.Cu")
    (at 124.841 58.42 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "Elevate_Logo:ElevateLogo" (layer "B.Cu")
    (at 124.841 75.565 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "Elevate_Logo:ElevateLogo" (layer "B.Cu")
    (at 124.841 69.85 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "Elevate_Logo:ElevateLogo" (layer "B.Cu")
    (at 124.841 64.135 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "Elevate_Logo:ElevateLogo" (layer "B.Cu")
    (at 124.841 81.28 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (gr_arc (start 113.411 84.455) (mid 111.614949 83.711051) (end 110.871 81.915)
    (layer "Edge.Cuts"))
  (gr_line (start 136.144 55.245) (end 113.411 55.245)
    (layer "Edge.Cuts"))
  (gr_arc (start 110.871 57.785) (mid 111.614949 55.988949) (end 113.411 55.245)
    (layer "Edge.Cuts"))
  (gr_line (start 136.144 84.455) (end 113.411 84.455)
    (layer "Edge.Cuts"))
  (gr_arc (start 138.684 81.915) (mid 137.940051 83.711051) (end 136.144 84.455)
    (layer "Edge.Cuts"))
  (gr_line (start 138.684 81.915) (end 138.684 57.785)
    (layer "Edge.Cuts"))
  (gr_arc (start 136.144 55.245) (mid 137.940051 55.988949) (end 138.684 57.785)
    (layer "Edge.Cuts"))
  (gr_line (start 110.871 57.785) (end 110.871 81.915)
    (layer "Edge.Cuts"))
  (zone (net 4) (net_name "GND") (layer "B.Cu") (hatch none 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.75) (thermal_bridge_width 0.75) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 119.888 64.516)
        (xy 131.445 64.516)
        (xy 131.445 82.169)
        (xy 119.888 82.296)
      )
    )
  )
)
